| CMSIS-DSP Verison 1.4.1 CMSIS DSP Software Library

- CMSIS
- CORE
- DSP
- RTOS API
- SVD

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
Vector Addition
Basic Math Functions

## Functions
void | arm_add_f32 (float32_t *pSrcA, float32_t *pSrcB, float32_t *pDst, uint32_t blockSize)
| Floating-point vector addition. More...
void | arm_add_q15 (q15_t *pSrcA, q15_t *pSrcB, q15_t *pDst, uint32_t blockSize)
| Q15 vector addition. More...
void | arm_add_q31 (q31_t *pSrcA, q31_t *pSrcB, q31_t *pDst, uint32_t blockSize)
| Q31 vector addition. More...
void | arm_add_q7 (q7_t *pSrcA, q7_t *pSrcB, q7_t *pDst, uint32_t blockSize)
| Q7 vector addition. More...

## Description

Element-by-element addition of two vectors.

        pDst[n] = pSrcA[n] + pSrcB[n],   0 <= n < blockSize.

There are separate functions for floating-point, Q7, Q15, and Q31 data types.

## Function Documentation

void arm_add_f32 | ( | float32_t * | pSrcA,
|  | float32_t * | pSrcB,
|  | float32_t * | pDst,
|  | uint32_t | blockSize
| ) |  |

Parameters

  [in] | *pSrcA | points to the first input vector
  [in] | *pSrcB | points to the second input vector
  [out] | *pDst | points to the output vector
  [in] | blockSize | number of samples in each vector

Returns
  none.

Examples:
  arm_dotproduct_example_f32.c, and arm_sin_cos_example_f32.c.

References blockSize.

Referenced by main().

void arm_add_q15 | ( | q15_t * | pSrcA,
|  | q15_t * | pSrcB,
|  | q15_t * | pDst,
|  | uint32_t | blockSize
| ) |  |

Parameters

  [in] | *pSrcA | points to the first input vector
  [in] | *pSrcB | points to the second input vector
  [out] | *pDst | points to the output vector
  [in] | blockSize | number of samples in each vector

Returns
  none.

Scaling and Overflow Behavior:

  The function uses saturating arithmetic. Results outside of the allowable Q15 range [0x8000 0x7FFF] will be saturated.

References __SIMD32, and blockSize.

void arm_add_q31 | ( | q31_t * | pSrcA,
|  | q31_t * | pSrcB,
|  | q31_t * | pDst,
|  | uint32_t | blockSize
| ) |  |

Parameters

  [in] | *pSrcA | points to the first input vector
  [in] | *pSrcB | points to the second input vector
  [out] | *pDst | points to the output vector
  [in] | blockSize | number of samples in each vector

Returns
  none.

Scaling and Overflow Behavior:

  The function uses saturating arithmetic. Results outside of the allowable Q31 range[0x80000000 0x7FFFFFFF] will be saturated.

References blockSize, and clip_q63_to_q31().

void arm_add_q7 | ( | q7_t * | pSrcA,
|  | q7_t * | pSrcB,
|  | q7_t * | pDst,
|  | uint32_t | blockSize
| ) |  |

Parameters

  [in] | *pSrcA | points to the first input vector
  [in] | *pSrcB | points to the second input vector
  [out] | *pDst | points to the output vector
  [in] | blockSize | number of samples in each vector

Returns
  none.

Scaling and Overflow Behavior:

  The function uses saturating arithmetic. Results outside of the allowable Q7 range [0x80 0x7F] will be saturated.

References __SIMD32, and blockSize.