| CMSIS-CORE Version 3.20 CMSIS-CORE support for Cortex-M processor-based devices

- CMSIS
- CORE
- DSP
- RTOS API
- SVD

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Enumerations Enumerator Groups Pages
Using CMSIS with generic ARM Processors

ARM provides CMSIS-CORE files for the supported ARM Processors and for various compiler vendors. These files can be used when standard ARM processors should be used in a project. The table below lists the folder and device names of the ARM processors.

Folder | Processor | Description
--- | --- | ---
".\Device\ARM\ARMCM0" | Cortex-M0 | Contains Include and Source template files configured for the Cortex-M0 processor. The device name is ARMCM0 and the name of the Device Header File <device.h> is <ARMCM0.h>.
".\Device\ARM\ARMCM0plus" | Cortex-M0+ | Contains Include and Source template files configured for the Cortex-M0+ processor. The device name is ARMCM0plus and the name of the Device Header File <device.h> is <ARMCM0plus.h>.
".\Device\ARM\ARMCM3" | Cortex-M3 | Contains Include and Source template files configured for the Cortex-M3 processor. The device name is ARMCM3 and the name of the Device Header File <device.h> is <ARMCM3.h>.
".\Device\ARM\ARMCM4" | Cortex-M4 | Contains Include and Source template files configured for the Cortex-M4 processor. The device name is ARMCM4 and the name of the Device Header File <device.h> is <ARMCM4.h>.
".\Device\ARM\ARMSC000" | SecurCore SC000 | Contains Include and Source template files configured for the SecurCore SC000 processor. The device name is ARMSC000 and the name of the Device Header File <device.h> is <ARMSC000.h>.
".\Device\ARM\ARMSC300" | SecurCore SC300 | Contains Include and Source template files configured for the SecurCore SC300 processor. The device name is ARMSC300 and the name of the Device Header File <device.h> is <ARMSC300.h>.

# Create generic Libraries with CMSIS

The CMSIS Processor and Core Peripheral files allow also to create generic libraries. The CMSIS-DSP Libraries are an example for such a generic library.

To build a generic Library set the define __CMSIS_GENERIC and include the relevant core_<cpu>.h CMSIS CPU & Core Access header file for the processor. The define __CMSIS_GENERIC disables device-dependent features such as the SysTick timer and the Interrupt System. Refer to Configuration of the Processor and Core Peripherals for a list of the available core_<cpu>.h header files.

Example:

The following code section shows the usage of the core_<cpu>.h header files to build a generic library for Cortex-M0, Cortex-M3, or Cortex-M4. To select the processor the source code uses the define CORTEX_M4, CORTEX_M3, or CORTEX_M0. By using this header file, the source code can access the functions for Core Register Access, Intrinsic Functions for CPU Instructions, Intrinsic Functions for SIMD Instructions [only Cortex-M4], and Debug Access.

#define __CMSIS_GENERIC /* disable NVIC and Systick functions */
#if defined (CORTEX_M4)
#include "core_cm4.h"
#elif defined (CORTEX_M3)
#include "core_cm3.h"
#elif defined (CORTEX_M0)
#include "core_cm0.h"
#elif defined (CORTEX_M0PLUS)
#include "core_cm0plus.h"
#else
#error "Processor not specified or unsupported."
#endif