| CMSIS-SVD Version 1.10 CMSIS System View Description

- CMSIS
- CORE
- DSP
- RTOS API
- SVD

- Main Page
- Usage and Description
- Reference

SVD File Validation

The quality of the available descriptions is key to the success of the CMSIS-SVD format. Aspects of quality are:

- Syntactical and structural compliance with the specified CMSIS-SVD format.
- Consistency and correctness.
- Completeness.
- Level of detail.

Automated checks are done on two levels:

1. The CMSIS-SVD Schema File: The schema file specifies the syntax and structure of an XML-based format. XML tools use the schema file for checking the syntactical and structural correctness of an XML file that claims compliance with a certain format. The schema file CMSIS-SVD_Schema_1_0.xsd can be found in the folder SVD of the CMSIS distribution.
2. SVD Conversion Utility: ARM provides the SVD Utility (SVDConv.exe) tool to check the semantics and consistency of the data contained in a CMSIS-SVD file. SVDConv is a command-line tool included in the CMSIS distribution. It is located in the SVD folder side by side with the CMSIS-SVD schema file. The SVDConv shall be used for checking CMSIS-SVD descriptions as well as for generating CMSIS-compliant device header files.
   - Usage Information:
     SVDConv provides usage information at the command line when invoked without arguments.
     SVDConv.exe
   - Consistency Check:
     SVDConv is performing a consistency of the CMSIS-SVD file passed as the first command-line argument. The checks go beyond syntactical tests as they can be performed using the CMSIS-SVD schema file in combination with XML validation tools. Errors and warnings are printed to the command line.
     SVDConv.exe myDevice.xml